Used in all multi-chip integrated circuits (SOT plastic packaging) the IC gold ball welding, complex production process, long life, stable performance, high qualified products.  
  
Voltage :4 - 8VDC  
  
Maximum current: = 30MA/5VDC  
  
Minimum sound pressure => 85db/10cm  
  
Resonant frequency of 2500 + - 300HZ  
  
Operating temperature: -20 ------ 70 degrees  
  
Weight: 2g  
  
The buzzer Usually most commonly used is 5V.

