**Product Name: 24-key Infrared Controller
Net Weight: 55g
Working Temperature:-20-60
Supply Voltage: DC12V
Max Load Current: 2A each color
Output: Three CMOS drain-open output
Connecting Mode: Common anode
Support Max 5 meter LED Strip**

**Package:**

**1 x IR Controller
1 x Remote
1 x User manual**

