**Product Name: 24-key Infrared Controller  
Net Weight: 55g  
Working Temperature:-20-60  
Supply Voltage: DC12V  
Max Load Current: 2A each color  
Output: Three CMOS drain-open output  
Connecting Mode: Common anode  
Support Max 5 meter LED Strip**

**Package:**

**1 x IR Controller  
1 x Remote  
1 x User manual**

